Main settings:

CG: 111mm

AIL: up 31mm/ dn 20mm

Mix Flap to AiI: 6up mm / 8dn mm

Ele: up 10mm / 11dn mm

Rud: up 8mm / 8dn mm

Mix Snapflap: Ele mm up, Flap+Ail mm dn

Butterfly: Flap 80°dn, Ail 16mm up, Ele 8mm dn